#
FRONT BRAKE (DISC) REMOVAL/INSTALLATION

BME041133980W02

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

3. After installation, depress the pedal a few times, rotate the wheel by hand, and verify that the brake does not drag.

.

1 | Flexible hose
2 | Caliper
3 | Disc pad (See Disc Pad Installation Note)
4 | Outer shim
5 | Inner shim
6 | Guide plate
7 | Mounting support
8 | Dust boot
9 | Disc plate (See Disc Plate Removal Note) (See Disc Plate Installation Note)

## Disc Plate Removal Note

1. Mark the wheel hub bolt and disc plate before removal for reference during installation.

## Disc Plate Installation Note

1. Remove any rust or grime on the contact face of the disc plate and wheel hub.

2. Install the disc plate and align the marks made before removal.

## Disc Pad Installation Note

1. Push the piston fully inward using the SST.

2. Install the disc pad.