#
FRONT COMBINATION LIGHT REMOVAL/INSTALLATION

BME091851030W02

1. Disconnect the negative battery cable.

2. Remove the front turn light.

3. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Bracket
4 | Front combination light

5. Install in the reverse order of removal.

6. Adjust the headlight aiming. (See HEADLIGHT AIMING.)