#
EMISSION SYSTEM LOCATION INDEX [AJ]

BME011600116205

Engine Room Side

Fuel Tank Side

1 | EGR valve (See EGR VALVE INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)) (See EGR VALVE INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))
2 | Purge solenoid valve (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [AJ].) (See PURGE SOLENOID VALVE INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513)) (See PURGE SOLENOID VALVE INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)))
3 | PCV valve (See PCV VALVE INSPECTION [AJ].)
4 | Oil separator
5 | Ventilation hose
6 | WU-TWC (See WARM-UP THREE-WAY CATALYTIC CONVERTER (WU-TWC) INSPECTION (EUROPEAN (L.H.D.) SPECS.) [AJ].)
7 | TWC
8 | Catch tank (See CATCH TANK INSPECTION [AJ].)
9 | Evaporative gas check valve (one-way) (See EVAPORATIVE GAS CHECK VALVE (ONE-WAY) INSPECTION [AJ].)
10 | BARO sensor (European (L.H.D.) specs.) (See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
EGR boost sensor (Australian, general (L.H.D. R.H.D.) specs.) (See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
11 | EGR boost sensor solenoid valve (Australian, general (L.H.D. R.H.D.) specs.) (See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).)
(See BAROMETRIC PRESSURE SENSOR/EGR BOOST SENSOR INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
12 | Rollover valve (See FUEL TANK INSPECTION [AJ])
13 | Charcoal canister (See CHARCOAL CANISTER INSPECTION [AJ].)