#
AUDIO CONTROL SWITCH INSPECTION

BME092000148W02

## Button Type

1. Measure the resistance and inspect for continuity between the audio control switch terminals using an ohmmeter.

  • If not as specified, replace the audio control switch.

## Lever Type

1. Measure the resistance between the audio control lever terminals using an ohmmeter.

  • If not as specified, replace the audio control lever.