#
FUEL FILTER COMPONENT DISASSEMBLY/ASSEMBLY [MZR-CD (RF Turbo)]

BME011420490203

1. Disconnect the negative battery cable.

2. Complete the "BEFORE SERVICE PRECAUTION". (See BEFORE SERVICE PRECAUTION [MZR-CD (RF Turbo)].)

3. Remove in the order indicated in the table.

1 | Connector
2 | Fuel hose
3 | Priming pump
4 | Fuel filter (See Fuel Filter Installation Note)
5 | Sedimentor switch (See Sedimentor Switch Installation Note)
6 | Drain plug
7 | Fuel warmer

4. Install in the reverse order of removal.

5. Complete the "AFTER SERVICE PRECAUTION". (See AFTER SERVICE PRECAUTION [MZR-CD (RF Turbo)].)

6. Start the engine and verify that fuel does not leak from the fuel system.

  • If fuel leaks, reassemble the fuel filter.

## Sedimentor Switch Installation Note

1. Apply a small amount of fuel to a new O-ring.

  • Tighten the sedimentor switch enough to the fuel filter by hand.

## Fuel Filter Installation Note

1. Apply a small amount of fuel to the fuel filter O-ring.

2. Tighten the fuel filter approx. 3/4 by hand after the O-ring contacts the priming pump.