#
JOINT SHAFT (AJ) DISASSEMBLY

BME031325700206

1. Disassemble in the order indicated in the table.

1 | Joint shaft (See Joint Shaft Disassembly Note.)
2 | Dust seal (differential side)
3 | Bearing (See Bearing Disassembly Note.)
4 | Dust seal (drive shaft side)
5 | Bracket
6 | Dust cover

## Joint Shaft Disassembly Note

1. Disassemble the joint shaft as shown in the figure.

  Caution

  • When disassembling the joint shaft, use a V block of adequate size to support the bearing inner race as well, otherwise the bearing inner race will be damaged and the bearing cannot be reused.

## Bearing Disassembly Note

1. Remove the bearing using the SSTs and a press.

  Caution

  • Do not damage the rubber part of the dust cover.