#
AIRFLOW DISTRIBUTION

BME071100000T03

## Front

• The ratio of air volume from each vent has been changed.

Airflow mode | Distribution (%)
--- | ---
Center and side vent | Front and rear heat | Defroster and side demister
VENT | 90 | 10 | 0
BI-LEVEL | 60 | 40 | 0
HEAT | 0 (20) | 80 (40) | 20 (40)
HEAT/DEF | 0 (20) | 50 (40) | 50 (40)
DEFROSTER | 0 (20) | 0 (0) | 100 (80)

  ( ) :
For the system which side vents are open.