#
NO.20 FUEL ODOR (IN ENGINE COMPARTMENT) [MZR-CD (RF Turbo)]

BME010300000W55

20 | FUEL ODOR (IN ENGINE COMPARTMENT)
--- | ---
DESCRIPTION | • Fuel smell or visible leakage.
POSSIBLE CAUSE | • Excessive fuel pressure • Fuel pressure limiter malfunction (built-in common rail) • Fuel leakage

  Warning
The following troubleshooting flow chart contains the fuel system diagnosis and repair procedures. Read the following warnings before performing the fuel system services:

  • Fuel vapor is hazardous. It can easily ignite, causing serious injury and damage. Always keep sparks and flames away from fuel.
  • Fuel line spills and leakage are dangerous. Fuel can ignite and cause serious injury or death and damage. Fuel can also irritate skin and eyes. To prevent this, always complete "BEFORE REPAIR PROCEDURE" and "AFTER REPAIR PROCEDURE" described in this manual.

Diagnostic Procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Visually inspect fuel leakage at fuel injector and fuel line. Is there any fuel leakage? | Yes | Service as necessary.
No | Go to next step.
2 | Visually inspect for damaged or cracked fuel filter. Is fuel filter okay? | Yes | Go to next step.
No | Replace fuel filter.
3 | Inspect fuel injector. (See FUEL INJECTOR INSPECTION [MZR-CD (RF Turbo)].) Is fuel injector okay? | Yes | Go to next step.
No | Repair or replace as necessary.
4 | Perform self-test function using WDS or equivalent. Turn engine switch to ON. Retrieve any DTC. Is DTC displayed? | Yes | DTC is displayed: Go to appropriate DTC test. Communication error message is displayed: Inspect for following: • Open circuit between PCM control relay and PCM terminal 53 or 79
• Open circuit PCM control relay and PCM terminal 69
• PCM control relay stuck open
• Open or poor GND circuit (PCM terminal 65, 85, 103 or 104)
• Poor connection vehicle body GND
No | No DTC is displayed: Remove and inspect common rail.
5 | Verify test results. • If okay, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)