#
CYLINDER HEAD BLOCK CONSTRUCTION [AJ]

BME011010300T04
• Aluminum alloy has been adopted on the cylinder block, and it consists of upper and lower cylinder blocks.
• Each cylinder is lined with a steel liner. Liner cutting and replacement is not possible.
• The cylinders are numbered 1, 2, 3 from the front along the right bank and 4, 5, 6 from the front along the left bank.

1 | Upper cylinder block
2 | Lower cylinder block
3 | Engine front
4 | Upper cylinder block
5 | Cast iron inserts