#
FOREWORD

BME090358000W01
• Always perform basic power window system inspection before troubleshooting.
• The table below lists unique troubleshooting for the automatic window return function with the jam-safe power window.

  Caution

  • The automatic window return may not operate properly if the following is performed on the front door.

  - The power window motor is operated without the door glass properly installed.
  - The door glass is replaced.
  - The glass run channel is replaced.
  - The power window regulator is removed or installed. If a new power window regulator is installed, however, the power window motor does not require resetting.