#
FRONT CLIMATE CONTROL UNIT INSTALLATION

BME074061190202

1. Install the front climate control unit to the center panel.

2. Pass each wire through the following routes then connect to front A/C unit.

3. Connect the front climate control unit connectors.

4. Install the meter hood.

5. Adjust the front climate control unit wire. (See FRONT CLIMATE CONTROL UNIT WIRE ADJUSTMENT.)

6. Connect the negative battery cable.