#
DTC 00 ERR01 OR 00:ER01

BME090266900W15

DTC 00 ERR01 or 00:Er01 | Cassette deck
DETECTION CONDITION | • Cassette deck cannot implement insert and eject commands.
POSSIBLE CAUSE | • Defective cassette tape (deformation, broken, or foreign material stuck/attached) • Cassette deck malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Is cassette tape able to be ejected? | Yes | Go to next step.
No | Replace cassette deck.
2 | INSPECT CASSETTE TAPE • Inspect condition of cassette tape where error has occurred. • Is cassette tape okay? | Yes | Go to next step.
No | Repair (remove foreign material) or replace cassette tape, then go to next step.
3 | INSPECT CASSETTE DECK • Clear DTC. • Insert and eject cassette tape with no defect. • Start on-board diagnostic test mode. • Is DTC 00 ERR01 or 00:Er01 displayed? | Yes | Replace cassette deck.
No | Troubleshooting completed.