#
ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [L3]

BME014018840202

  Warning

  • When the engine is hot, it can badly burn. Turn off the engine and wait until it is cool before removing the ECT sensor.

1. Drain the engine coolant.

2. Disconnect the ECT sensor connector.

3. Remove the ECT sensor.

4. Install in the reverse order of removal.

Tightening torque

  10-14 N·m
  {1.02-1.42 kgf·m, 7.38-10.32 ft·lbf}

5. Refill the engine coolant.