#
WHEEL HUB, HUB SPINDLE REMOVAL/INSTALLATION

BME031205000203

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | ABS sensor (with ABS)
2 | Hub cap
3 | Locknut (See Locknut Removal Note.) (See Locknut Installation Note.)
4 | Brake caliper component (See Brake Caliper Removal Note.)
5 | Disc plate (See Disc Plate Removal Note.) (See Disc Plate Installation Note.)
6 | Wheel hub and ABS sensor rotor (with ABS)
7 | ABS sensor rotor (with ABS) (See ABS Sensor Rotor (vehicles with ABS) Removal Note.) (See ABS Sensor Rotor (vehicles with ABS) Installation Note.)
8 | Hub bolt (See Hub Bolt Removal Note.) (See Hub Bolt Installation Note.)
9 | Wheel hub
10 | Bolt
11 | Parking brake cable
12 | Rear brake component
13 | Hub spindle

## Locknut Removal Note

1. Raise the staked portion of the locknut using a small cape chisel and a hammer.

2. Lock the hub by applying the brakes.

3. Remove the locknut.

## ABS Sensor Rotor (vehicles with ABS) Removal Note

  Note

  • The sensor rotor does not need to be removed unless it is being replaced.

1. Remove the sensor rotor using a chisel.

## ABS Sensor Rotor (vehicles with ABS) Installation Note

1. Set the SST as shown in the figure.

  Caution

  • Position the SST so that the portion marked B faces downward.

2. Press on the new sensor rotor using the SST and a press.

## Locknut Installation Note

1. Install a new locknut and stake it as shown in the figure.