#
INPUT/TURBINE SPEED SENSOR INSPECTION [JA5A-EL]

BME051721550201

## On-Vehicle Inspection

1. Disconnect the terminal component No.2 connector.

2. Measure resistance between the terminals E and F.

  • If not within the specification, inspect the input/turbine speed sensor. (See Individual Part Inspection.)

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Connect the terminal component No.2 connector.

## Individual Part Inspection

1. Remove the input/turbine speed sensor. (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5A-EL].)

2. Measure resistance between the terminals of the input/turbine speed sensor.

  • If not within the specification, replace the input/turbine speed sensor.
  • If it is normal, replace the harness.

Resistance (ATF temperature: 20 °C {68 °F})

  513-627 ohms

3. Install the input/turbine sensor. (See INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5A-EL].)