#
MANUAL TRANSAXLE SPECIFICATIONS [G15M-R]

BME050000000T10

Item | Specifications
--- | ---
Transaxle type | G15M-R
Engine type | L3
Transaxle control | Floor-shift
Operation system | Rod
Shift assist | Forward | Synchromesh
Reverse | Selective sliding and synchromesh
Gear ratio | 1st | 3.307
2nd | 1.842
3rd | 1.310
4th | 0.970
5th | 0.755
Reverse | 3.166
Final gear ratio | 4.588
Oil | Grade | API service GL-4 or GL-5
Viscosity | All season | SAE 75W-90
Above 10°C {50°F} | SAE 80W-90
Capacity (approximate quantity) (L {US qt, Imp qt}) | 2.70 {2.85, 2.38}