#
NO.3 VEHICLE MOVES IN P POSITION, OR PARKING GEAR DOES NOT DISENGAGE WHEN P IS DISENGAGED [JA5A-EL]

BME050301030239

3 | Vehicle moves in P position, or parking gear does not disengage when P is disengaged
DESCRIPTION | • Vehicle rolls on a downward slope in P position. • Tires are locked when P position is disengaged. Vehicle does not move in D, S, L ranges, and R position when the accelerator pedal is depressed, and the engine remains in a stalled condition.
POSSIBLE CAUSE | 1. Parking mechanism malfunction (May have effect on noise or shock from transaxle) 2. Improper adjustment of selector lever 3. If vehicle moves in N position, perform No.2 "VEHICLE MOVES IN N POSITION"

  Note

  • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.