#
PID/DATA MONITOR INSPECTION [JA5A-EL]

BME050218901232

1. Connect the WDS or equivalent to the DLC-2.

2. Turn the ignition switch to the ON position.

3. Measure the PID value.

  Note

  • Perform part inspection for the output device after TCM inspection.
  • The PID/DATA MONITOR function monitors the calculated value of the input/output signals in the TCM. Therefore, if a monitored value of an output device is out of specification, it is necessary to inspect the monitored value of the input device related to the output device control. Since an output device malfunction is not directly indicated as a malfunction of the monitored value for the output device, it is necessary to inspect the output device individually using the simulation function, or similar.

PID/DATA MONITOR AND RECORD function table

Monitor item (Definition) | Unit/Condition | Condition/Specification | Action | TCM terminal
--- | --- | --- | --- | ---
24B_Duty (2-4 brake solenoid vale) | % | N position: 0% 2GR, 4GR or 5GR: 99% | Inspect the 2-4 brake solenoid valve. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | 2V
BOO TCM (Brake switch) | on/off | Brake pedal depressed: on Brake pedal released: off | Inspect the brake switch. | 1U
PNP_TCM (TR switch (P/N position switch)) | Drive/Neutral | P or N position: Neutral R position and all ranges: Drive | Inspect the TR switch. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | -
FAT (FAT terminal (DLC)) | on/off | No DTC output: off DTC output: on-off | Inspect the DLC FAT terminal and TCM connector terminal 1Q. | 1Q
GEAR (Calculated gear range in TCM) | 1/2/3/4/5 | 1GR: 1 2GR: 2 3GR: 3 4GR: 4 5GR: 5 | Inspect the following PIDs: THOP, TSS | -
HC_Duty (High clutch solenoid valve) | % | N position: 0% 3GR, 4GR or 5GR: 99% | Inspect the high clutch solenoid valve. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | 2U
LPS (Pressure control solenoid) | % | Ignition switch ON: 0% Idle: 0-100% | Inspect the pressure control solenoid. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | 2Y
N_SFT (Neutral shift solenoid valve) | on/off | N position: off R position inhibition control: on | Inspect the main relay. (See RELAY INSPECTION.) Inspect the battery. (See BATTERY INSPECTION.) | 2D
OSS (Intermediate sensor | RPM | Idle: 700-800 RPM | Inspect the intermediate sensor. (See INTERMEDIATE SENSOR INSPECTION [JA5A-EL].) | 1K, 1X
RDCN_TIM (Reduction timing solenoid valve) | on/off | N position: off D range: on | Inspect the reduction timing solenoid valve. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | 2G
RPM_TCM (Engine speed) | RPM | Idle: 700-800 RPM | Inspect the TCM. (See TCM INSPECTION [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See TCM INSPECTION [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).) | -
SSA/SS1 (Shift solenoid A) | on/off | N position: on D range 3GR: off | Inspect shift solenoid A. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | -
SSB/SS2 (Shift solenoid B) | on/off | N position: on D range 4GR: off | Inspect shift solenoid B. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | -
SSC/SS3 (Shift solenoid C) | on/off | N position: on D range 2GR: off | Inspect shift solenoid C. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | -
TAT (TAT terminal) | on/off | Open terminal TAT: on Short terminal TAT: off | Inspect the DLC TAT terminal and TCM connector terminal 1A. | 1A
TCCC (TCC solenoid valve) | % | TCC operating: 0-100% TCC non operating: 0% | Inspect the TCC solenoid valve. (See SOLENOID VALVE INSPECTION [JA5A-EL].) | 2S
TCIL (HOLD indicator light) | on/off | HOLD mode: on Other modes: off | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [JA5A-EL].) | 1E
TCS (HOLD switch) | on/off | HOLD switch pressed: on Other: off | Inspect the HOLD switch. (See HOLD SWITCH INSPECTION [JA5A-EL].) | 2I
TFT (ATF temperature) | °C, °F | ATF 20 °C{68 °F}: 20 °C {68 °F} ATF 60 °C {140 °F}: 60 °C {140 °F} | Inspect the TFT sensor. (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5A-EL].) | 1B, 1F
TFTV (ATF temperature signal voltage) | V | ATF 20 °C {68 °F}: 1.55 V ATF 60°C {140 °F}: 0.7 V | Inspect the TFT sensor. (See TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR INSPECTION [JA5A-EL].) | 1B, 1F
THOP (Throttle position) | % | CTP: 0% WOT: 100% | Inspect the TCM. (See TCM INSPECTION [JA5A-EL] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).) (See TCM INSPECTION [JA5A-EL] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).) | -
TRD (TR switch [D range]) | on/off | D range: on Other ranges and all positions: off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].) | 1Z
TRL (TR switch [2 range]) | on/off | 2 range: on Other ranges and all positions: off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].) | 2C
TRR (TR switch [R position]) | on/off | R position: on Other positions and all ranges: off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].) | 1W
TRS (TR switch [3 range]) | on/off | 3 range: on Other ranges and all positions: off | Inspect the TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL].) | 1AA
TSS (Input/turbine speed sensor) | RPM | Idle: 700-800 RPM | Inspect the input/turbine speed sensor. (See INPUT/TURBINE SPEED SENSOR INSPECTION [JA5A-EL].) | 1N, 2F
VPWR_TCM (Battery voltage) | V | IG ON: B+ Idle: 13-14 V | Inspect the main relay. (See RELAY INSPECTION.) | 1P
VSS_TCM (Vehicle speed) | KPH, MPH | Vehicle speed 20 km/h {12.5 mph}: 20 KPH {12.5 MPH} Vehicle speed 40 km/h {25 mph}: 40 KPH {25 MPH} | Inspect the vehicle speedometer sensor. (See VEHICLE SPEED SENSOR (VSS) INSPECTION [JA5A-EL].) | 1V, 1M