#
DTC P0841 [FN4A-EL]

BME050201030234

DTC P0841 | Oil pressure switch circuit malfunction
--- | ---
DETECTION CONDITION | • If each of DTC P0731, P0732, P0733 and P0734 are not detected and 10 s or more passed, the PCM determines that there is a malfunction.

  - When all conditions below are satisfied while driving in 1GR, 2GR or 3GR.

  • ATF temperature 20 °C {68 °F} or more.
  • Oil pressure switch OFF
  • Revolution ratio of forward clutch drum revolution to differential gear case revolution below 0.91 or more than 3.08.
  • None of the following present: DTC P0500, P0705, P0706, P0711, P0712, P0713, P0715, P0751, P0752, P0753, P0756, P0757, P0758, P0761, P0762, P0763, P0766, P0767, P0768, P0771, P0772, P0773

  - When all conditions below are satisfied while driving in 4GR.

  • ATF temperature 20 °C {68 °F} or more.
  • Oil pressure switch ON
  • Revolution ratio of forward clutch drum revolution to differential gear case revolution below 0.64 or more than 0.82.
  • None of the following present: DTC P0500, P0705, P0706, P0711, P0712, P0713, P0715, P0751, P0752, P0753, P0756, P0757, P0758, P0761, P0762, P0763, P0766, P0767, P0768, P0771, P0772, P0773

Diagnostic support note:
• This is a continuous monitor (CCM).
• The MIL illuminates if the PCM detects the above malfunction condition in two consecutive drive cycles or in one drive cycle while the DTC for the same malfunction has been stored in the PCM.
• A PENDING CODE is not available.
• FREEZE FRAME DATA is not available.
• The HOLD indicator light flashes.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • Oil pressure switch malfunction • Open circuit between oil pressure switch terminal A and PCM terminal 3T • Short to ground between oil pressure switch terminal A and PCM terminal 3T • Damaged connector between oil pressure switch and PCM • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has the FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | INSPECT OIL PRESSURE SWITCH CONNECTOR FOR POOR CONNECTION • Disconnect the shift oil pressure switch connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is the connection normal? | Yes | Go to the next step.
No | Repair or replace the connector and/or terminal, then go to Step 7.
3 | INSPECT CONTINUITY • Inspect for continuity between oil pressure switch (part-side) terminal A and body ground. • Is there continuity? | Yes | Replace the oil pressure switch, then go to Step 7. (See OIL PRESSURE SWITCH REMOVAL/INSTALLATION [FN4A-EL].)
No | Go to the next step.
4 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Disconnect the PCM connector. • Inspect for poor connection (such as damaged/pulled-out pins, corrosion). • Is the connection normal? | Yes | Go to the next step.
No | Repair or replace the connector and/or terminals, then go to Step 7.
5 | INSPECT OIL PRESSURE SWITCH CIRCUIT FOR OPEN • Inspect for continuity between PCM (wiring harness-side) terminal 3T and ATX (wiring harness-side) terminal A. • Is there continuity between the terminals? | Yes | Go to the next step.
No | Repair or replace the wiring harness, then go to Step 7.
6 | INSPECT PCM CIRCUIT FOR SHORT TO GROUND • Turn the ignition switch to the LOCK position. • Inspect for continuity between PCM (wiring harness-side) terminal 3T and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness, then go to the next step.
No | Replace the oil pressure switch, then go to the next step. (See OIL PRESSURE SWITCH REMOVAL/INSTALLATION [FN4A-EL].)
7 | VERIFY TROUBLESHOOTING OF DTC P0841 COMPLETED • Make sure to reconnect all the disconnected connectors. • Clear the DTC from the memory using the WDS or equivalent. • Drive the vehicle and make sure that gears shift smoothly from 1GR to 4GR. • Are any DTCs present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L3].)
No | No concern is detected. Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the "After Repair Procedure". (See AFTER REPAIR PROCEDURE [FN4A-EL].) • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See DTC TABLE [FN4A-EL].)
No | DTC troubleshooting completed.