#
FRONT CROSSMEMBER REMOVAL/INSTALLATION

BME021334800201

1. Remove the front pipe. (L3) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3].)

Remove the front pipe and TWC. (AJ) (See EXHAUST SYSTEM REMOVAL/INSTALLATION [AJ].)

Remove the flexible pipe. (MZR-CD (RF Turbo))(See EXHAUST SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Remove the extension bar and change control rod. (L3 MTX only)

3. Remove the engine mount member.

4. Remove the steering gear and linkage. (See STEERING GEAR AND LINKAGE REMOVAL/INSTALLATION.)

5. Remove the transverse member.

6. Remove the front lower arm.

7. Remove in the order indicated in the table.

1 | Stabilizer control link nut
2 | No.1 engine mount center bolt
3 | No.1 engine mount bracket (MZR-CD (RF Turbo) only)
4 | Crossmember component (See Crossmember Component Removal Note.)
5 | Front stabilizer
6 | No.1 engine mount
7 | Front crossmember

8. Install in the reverse order of removal.

9. Inspect the front wheel alignment if necessary.

## Crossmember Component Removal Note

1. Support the crossmember using a jack and remove the bolts and nuts.

2. Remove the crossmember component.