#
TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL]

BME051719200202

## Operating Inspection

1. Verify that the starter operates only when the ignition switch is turned to the START position with the selector lever in the P or N position.

  • If there is any malfunction, adjust the TR switch.

2. Verify that the back-up lights illuminate when shifted to the R position with the ignition switch at the ON position.

  • If there is any malfunction, adjust the TR switch.

3. Verify that the positions of the selector lever and the indicator are aligned.

  • If there is any malfunction, adjust the TR switch.

## Inspection of Continuity

  Caution

  • Water or foreign material entering the connector can cause a poor connection or corrosion. Be sure not to spill water or foreign material on the connector when disconnecting it.

1. Disconnect the negative battery cable.

2. Remove the splash shield.

3. Disconnect the TR switch connector.

4. Inspect the TR switch for continuity.

  • If there is any malfunction, adjust the TR switch and go to Step 5.

5. Reinspect the TR switch for continuity.

  • If there is any malfunction, replace the TR switch. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FN4A-EL].)

6. Connect the TR switch connector.

7. Install the splash shield.

8. Connect the negative battery cable.