#
CIGARETTE LIGHTER REMOVAL/INSTALLATION

BME092067000201

1. Disconnect the negative battery cable.

2. Remove the meter hood.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Cigarette lighter plug
2 | Screw
3 | Connector
4 | Socket (See Socket Removal Note.)
5 | Ring (See Ring Removal Note.)
6 | Cigarette lighter mounting panel

## Socket Removal Note

1. Turn the socket while pushing the protrusion of the ring through the hole of the socket with a tape-wrapped flathead screwdriver.

2. Push the socket forward.

3. Turn the socket clockwise to the position shown to pull it forward.

## Ring Removal Note

1. Pull the ring forward while compressing the hooks.