#
FRONT SEAT BELT REMOVAL/INSTALLATION

BME081157630W01

  Warning

  • Handling the front seat belt (pre-tensioner seat belt) improperly can accidentally deploy the pre-tensioner, which may seriously injure you. Read SERVICE WARNINGS before handling the front seat belt. (See SERVICE WARNINGS.)

  Caution

  • The ELR has a spring that will unwind if the retractor's cover is removed. The spring cannot be rewound by hand. If this occurs, the ELR will not work properly. Therefore, do not disassemble the retractor.

1. Turn the ignition switch to LOCK position.

2. Disconnect the negative battery cable and wait for more than 1 minute.

3. Remove the B-pillar lower trim.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Verify that the air bag system warning light illuminates for approximately 6 seconds and then goes off.

  • If the air bag system warning light does not operate in the manner described above, there are malfunction in the system. Inspect the system using the on-board diagnostic function.

1 | Connector (with pre-tensioner seat belt)
2 | Anchor cover
3 | Front seat belt