#
FRONT POWER WINDOW REGULATOR REMOVAL/INSTALLATION

BME091258560201

1. Disconnect the negative battery cable.

2. Remove the front door glass. (See FRONT DOOR DISASSEMBLY/ASSEMBLY.)

3. Disconnect the front power window regulator connector.

4. Remove the nuts, then remove the front power window regulator.

Tightening torque

  6.87-9.80 N·m {70-100 kgf·cm, 60.8-86.7 in·lbf}

5. Install in the reverse order of removal.

6. Reset the power window motor. (driver's side only) (See DRIVER-SIDE POWER WINDOW MOTOR RESETTING.)

  • If a new power window regulator is installed, however, the power window motor does not require resetting.