#
SHIFT-LOCK INSPECTION

BME051830000201

1. Turn the ignition switch to the ON position.

2. Verify that the selector lever is in P position.

3. Without the brake pedal depressed, verify that the selector lever cannot be shifted from P position.

4. Depress the brake pedal and verify that the selector lever can be shifted from P position.

  • If there is any malfunction, inspect the P position switch continuity and/or shift-lock relay, shift-lock solenoid continuity.