#
INTERMEDIATE SENSOR REMOVAL/INSTALLATION [JA5A-EL]

BME051719200214

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)

2. Remove the intermediate sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

3. Install the intermediate sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

4. Install the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)