#
NO.10 FREQUENT SHIFTING [FN4A-EL]

BME050301030214

10 | Frequent shifting
DESCRIPTION | • Downshifting occurs suddenly even when accelerator pedal is depressed slightly in D, S, L ranges except HOLD mode.
POSSIBLE CAUSE | • The malfunctioning circuit is basically the same as No.9 "ABNORMAL SHIFTING". However, a malfunction of the input signal to the TP sensor, input/turbine speed sensor, vehicle speed sensor (including the sensor GND, sensor harness and connector), or clutch slippage (clutch stuck, low pressure in line) may also be the cause.