#
COMBINATION SWITCH REMOVAL/INSTALLATION

BME091866120201

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

4. Remove the column cover.

5. Remove the clock spring. (See CLOCK SPRING REMOVAL/INSTALLATION.)

6. Remove in the order indicated in the table.

7. Install in the reverse order of removal.

1 | Connector
2 | Screw
3 | Combination switch