#
ENGINE COOLANT LEVEL INSPECTION

BME011215001W01

  Warning

  • Remove and install all parts when the engine is cold, otherwise they can cause severe burns or serious injury.
  • Turn off the engine and wait until it is cool. Even then, be very careful when removing the cap. Wrap a thick cloth around it and slowly turn it counterclockwise 2.5 turns. Step back while the pressure escapes.
  • When you are sure all the pressure is gone, turn the cap using the cloth, and remove it.

1. Verify that the coolant level in the coolant reservoir is between the F and L marks.

2. If the engine coolant level is below L mark, remove the cooling system cap and add engine coolant.