#
GENERATOR CONSTRUCTION [AJ]

BME011700000T09

## Structure

• The one-way clutch has been eleminated from the generator pulley due to the reduced drive belt pulsation from the improved engine performance.
• Due to the doubled Y connection circuit, the operation noise has been reduced and the output has become higher.

1 | Stator coil
2 | Generator
3 | Power transistor
4 | PCM
5 | Ignition switch
6 | Generator warning light
7 | Battery