#
DTC 35

BME010266350207

DTC 35 | TR switch
--- | ---
DETECTION CONDITION | • Voltage detected at cruise actuator connector terminal F is not approximately 0 V.
POSSIBLE CAUSE | • Cruise actuator malfunction • Starter malfunction • TR switch malfunction • Open circuit in wiring harness between ignition switch and TR switch • Open circuit in wiring harness between cruise actuator and TR switch

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT TR SWITCH • Inspect TR switch. (See TRANSAXLE RANGE (TR) SWITCH INSPECTION [FN4A-EL], TRANSAXLE RANGE (TR) SWITCH INSPECTION [JA5A-EL]) • Is TR switch okay? | Yes | Go to next step.
No | Replace TR switch. (See TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [FN4A-EL], TRANSAXLE RANGE (TR) SWITCH REMOVAL/INSTALLATION [JA5A-EL])
* 2 | INSPECT WIRING HARNESS BETWEEN TR SWITCH AND GROUND FOR CONTINUITY • Disconnect TR switch connector. • Is there continuity between TR switch connector terminal B and ground? | Yes | Go to next step.
No | Repair wiring harness (TR switch-starter) or inspect starter.
* 3 | INSPECT WIRING HARNESS BETWEEN CRUISE ACTUATOR AND TR SWITCH FOR CONTINUITY • Disconnect cruise actuator connector. • Is there continuity between cruise actuator connector terminal F and TR switch connector terminal H? | Yes | Replace cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION)
No | Repair wiring harness. (cruise actuator-TR switch)