#
ROOF MOLDING REMOVAL/INSTALLATION

BME091650620201

## Without Roof Rail

1. Remove the headliner.

2. Remove the shock absobing pad.

3. Remove the right side rear cooler duct No.1.

4. Remove the nuts, and then pull the molding up.

5. Install in the reverse order of removal.

## With Roof Rail

1. Remove the roof rail.

2. Remove the roof molding from roof rail.

3. Install in the reverse order of removal.