#
SUSPENSION

BME025000000W01

## Suspension

Item | Fuel gauge indication
--- | ---
Empty | 1/4 | 1/2 | 3/4 | Full
Front wheel alignment (unloaded*1) | Total toe-in | (mm {in}) | Rim inner: 1±3 {0.04±0.12}, Tire: 2±4 {0.08±0.16}
(degree) | 0°11'±0°22'
Maximum steering angle | Inner | 37°06'±3°
Outer | 32°±3°
Camber angle*2 |  | -0°12'±1° | -0°13'±1° | -0°14'±1°
Caster angle*2 |  | 1°57'±1° | 1°58'±1° | 1°59'±1° | 2°00'±1° | 2°02'±1°
Steering axis inclination (reference value) |  | 11°08' | 11°09' | 11°10' | 11°11'
Rear wheel alignment (unloaded*1) | Total toe-in | (mm {in}) | Rim inner: 2±3 {0.08±0.12}, Tire: 3±4 {0.12±0.16}
(degree) | 0°17'±0°22'
Camber angle (reference value) | -1°±1°

  *1 :
Engine coolant and engine oil are at specified levels. Spare tire, jack and tools are in designated positions.
  *2 :
Difference between left and right must not exceed 1°30'.

## Wheels and Tires

Item | Specification
--- | ---
Standard tire | Tire | Size | 215/60R16 95H
Air pressure (kPa {kgf/cm2, psi}) | Front | Up to 4 persons | 240 {2.4, 35}
More than 4 persons to full load | 250 {2.6, 37}
Rear | Up to 4 persons | 240 {2.4, 35}
More than 4 persons to full load | 290 {3.0, 43}
Remaining tread | Standard tire | (mm {oz}) | 1.6 {0.063}
Snow tire | 50% of tread
Wheel | Size | 16 x 6 1/2JJ
Material | Steel | Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Runout limit | (mm {in}) | Horizontal | 2.5 {0.098} | 2.0 {0.079}
Vertical | 1.5 {0.059}
Unbalance limit (at rim edge) | (g {oz}) | 8 {0.28}
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8-147.0 {11.00-14.98, 79.6-108.4}
Temporary spare tire (Karakuri models) | Tire | Size | T145/80D 16
Air pressure | (kPa {kgf/cm2,psi}) | 420 {4.2, 60}
Wheel | Size | 16 x 4T
Material | Steel
Offset | (mm {in}) | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}
Wheel nut tightening torque | (N·m {kgf·m, ft·lbf}) | 107.8-147.0 {11.00-14.98, 79.6-108.4}