#
DRIVELINE/AXLE SPECIFICATIONS

BME030001018102

Item | Specifications
--- | ---
L3 | AJ | MZR-CD (RF TURBO)
MTX | ATX | ATX | MTX
Front axle | Bearing type | Angular ball bearing
Rear axle | Bearing type | Angular ball bearing
Drive shaft | Joint type | Wheel side | Bell joint
Differential side | Double offset joint | Tripod joint (With roller cassette) | Tripod joint (With roller cassette) | Double offset joint
Shaft diameter | (mm {in}) | 30.0 {1.18} | 25.0 {0.98} | Left side: 24.0 {0.94} Right side: 30.0 {1.18} | 30.0 {1.18}
Joint shaft | Shaft diameter | (mm {in}) | 29.0 {1.14} | 29.0 {1.14} | 38.0 {1.50} | 41.0 {1.61}