#
REAR DRAIN HOSE INSTALLATION

BME091569922202

  Caution

  • If the rear drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the rear drain hose. Fix any problem if found.

1. Apply soapy water to the rear drain hose inserting area.

2. Insert one end (the wider side) of the rear drain hose into the sunroof frame.

3. Install the rear drain hose to the clips parallel to the pillar and free of slack.

4. Insert the rear drain hose joint into the rear pillar inner hole.

5. Install the trunk side trim.

6. Install the headliner.