#
REAR FENDER PANEL INSTALLATION

BME098074100702

1. When joining the new and old parts, temporarily install and fit the new part in position, measure each dimension according to the body dimension drawing, then adjust the position to align it to the standard dimension.

2. After trial-fitting new parts, make sure the related parts fit properly.

3. Before installing new parts, apply body sealer to the wheel arch line.