#
VARIABLE SWIRL CONTROL (VSC) VALVE ACTUATOR INSPECTION [MZR-CD (RF Turbo)]

BME011313110201

1. Disconnect the vacuum hose from the VSC solenoid valve.

2. Connect a vacuum pump to the vacuum hose.

3. Apply vacuum and verify that the rod moves as specified.

  • If not as specified, replace the intake manifold.

Specification

Vacuum (kPa {mmHg, inHg}) | Rod movement
--- | ---
Below -20 {-150, -5.9} | Starts to move
Above -69.4 {-521, -20.5} | Fully pulled