#
SPARE TIRE CARRIER OPERATION

BME091656100T12

1. When the jack handle is rotated, the cable is wound clockwise and the spare tire is raised. Until the anchor is completely seated, the spare tire lever is held between links A and B and cannot be removed.

1 | Jack handle
2 | Cable
3 | Ring
4 | Anchor
5 | Spare tire
6 | Spare tire lever
7 | Link A
8 | Link B
9 | Up

2. When the cable is wound until just before the tire is secured, the ring attached to the cable contacts link A.

1 | Ring
2 | Cable
3 | Anchor
4 | Link A
5 | Up

3. The spare tire lever can be removed when the anchor is completely seated, and links A and B are connected and pushed outward, locking the anchor and tire in place. If the cable should break in the section marked C, the cap prevents links A and B from moving in the directions marked D.

1 | Spare tire lever
2 | Cap
3 | Link A
4 | Link B
5 | Cable
6 | Lock
7 | Anchor
8 | Ring
9 | Socket
10 | Push
11 | Remove