#
OIL PRESSURE SWITCH REMOVAL/INSTALLATION [FN4A-EL]

BME051719200208

  Warning

  • When the transaxle and ATF are hot, they can badly burn. Turn off the engine and wait until they are cool before replacing ATF.

1. Disconnect the negative battery cable.

2. Remove the under cover.

3. Disconnect the wiring harness component connector.

4. Remove the oil pressure switch.

5. Install the oil pressure switch.

Tightening torque

  17.1-22.1 N·m {1.75-2.25 kgf·m, 12.7-16.2 ft·lbf}

6. Connect the oil pressure switch connector.

7. Install the under cover.

8. Connect the negative battery cable.