#
CLUTCH COVER INSPECTION

BME051016410201

1. Measure the wear of the diaphragm spring fingers.

  • If it exceeds the maximum specification, replace the clutch cover.

Maximum depth

  0.6 mm {0.024 in}

2. Measure the flatness of the pressure plate with a straight edge and a feeler gauge.

  • If it exceeds the maximum specification, replace the clutch cover.

Maximum clearance

  0.3 mm {0.012 in}

3. When checking the diaphragm spring fingers, mount a dial indicator on the cylinder block.

4. Rotate the flywheel and check for misaligned diaphragm spring fingers.

  • If it exceeds the maximum specification, replace the clutch cover.

Maximum height difference

  0.6 mm {0.024 in}