#
PULSATION DAMPER INSPECTION [L3]

BME011420180202

1. Complete the "BEFORE SERVICE PRECAUTION". (See BEFORE SERVICE PRECAUTION [L3].)

2. Remove the pulsation damper. (See PULSATION DAMPER REMOVAL/INSTALLATION [L3].)

3. Visually inspect the pulsation damper for damage and cracks. Also verify that there is no extreme rust which will cause fuel leakage.

  • If either is observed, replace the pulsation damper.

4. Complete the "AFTER SERVICE PRECAUTION". (See AFTER SERVICE PRECAUTION [L3].)