#
TRANSMITTER BATTERY INSPECTION

BME0914675DYW02

  Caution

  • ID code is transmitted for about 0.3 seconds after pushing the transmitter button. Therefore pushing the button again within about 0.3 seconds after pushing it is not applicable. Always push the button once every second.
  • Since the battery voltage does not drop fully if the button is pushed only four times or less, it can not be properly examined to see whether it is good or bad. Always push the button five times.

  Note

  • Since a correct measurement can not be obtained if the battery temperature is low, make sure the battery has been at 18 °C {64 °F} or more for at least 30 minutes before reinspecting when a measurement value is under the standard voltage.

1. Push any button of the transmitter five times every a second.

2. Remove the battery.

  Caution

  • The battery voltage recovers gradually after pushing the transmitter button. The standard voltage is the voltage recovered after a minute after pushing the button. If the inspection is not performed under this condition, a correct measurement can not be obtained. Always measure the voltage a minute after pushing the button.

3. Wait for a minute since the button is last pushed and measure the battery voltage.

Standard voltage

  2.7 V