#
CAMSHAFT POSITION (CMP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME014018230W02

  Caution

  • When foreign material, such as iron chips, gets on the CMP sensor, it can cause abnormal output from the sensor because of flux turbulence and adversely affect engine control. Be sure there is no foreign material on the CMP sensor when replacing.
  • Do not forcefully pull the wiring harness of the CMP sensor. Doing so will break the harness.

1. Disconnect the negative battery cable.

2. Remove the engine cover.

3. Remove in the order indicated in the table.

1 | CMP sensor installation bolt
2 | CMP sensor
3 | O-ring (See O-ring Installation Note)

4. Install in the reverse order of removal.

## O-ring Installation Note

1. Apply engine oil to new O-ring thinly and install it as does not damage.