#
FUEL TANK INSPECTION [MZR-CD (RF Turbo)]

BME011442110204

  Caution

  • Disconnecting/connecting the quick release connector without cleaning it may possibly cause damage to the fuel pipe and quick release connector. Always clean the quick release connector joint area before disconnecting/connecting using a cloth or soft brush, and make sure that it is free of foreign material.

  Note

  • This inspection is for two rollover valves integrated in the fuel tank.

1. Disconnect the fuel hose and the fuel gauge sender unit connector.

2. Remove the fuel tank with the fuel pump unit. (See FUEL TANK REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Plug the fuel pipe of the fuel pump unit.

4. Plug port C.

5. Level the fuel tank.

6. Blow through port B and verify that there is airflow from port A.

  • If there is no airflow, replace the fuel tank.
  • If there is airflow, turn the fuel tank upside-down, and proceed to Step 7.

7. Blow through port B and verify that there is no airflow from port A.

  • If there is airflow, replace the fuel tank.