#
BONNET REMOVAL/INSTALLATION

BME091052310201

  Warning

  • Removing the bonnet without supporting it can be dangerous. The bonnet may fall and injure you. Always perform the following proceduer with at least another person.

1. Disconnect the windshield washer hose.

2. To remove the bonnet hinge, remove the front fender panel.

3. To remove the bonnet lock, remove the radiator grille.

4. To remove the bonnet release cable, remove the driver-side mud guard.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. Adjust the bonnet. (See BONNET ADJUSTMENT.)

1 | Bonnet insulator
2 | Shroud seal weatherstrip
3 | Parting seal weatherstrip
4 | Bonnet
5 | Bonnet hinge
6 | Bonnet stay
7 | Bonnet lock
8 | Bonnet release lever
9 | Bonnet release cable