#
INSPECTION OF SST (DEPLOYMENT TOOL)

BME081001046202
• Use the SST (Deployment tool) to deploy a live (undeployed) air bag module or pre-tensioner seat belt before disposing of it.
• Before using the SST (Deployment tool), inspect its operation.

## Inspection Procedure

1. Follow the steps below to verify that the SST (Deployment tool) is operating correctly.

  • If not as specified, do not use the SST (Deployment tool) because it may cause the air bag module or pre-tensioner seat belt to unexpectedly deploy upon connection to the air bag module or pre-tensioner seat belt.

Step | Inspection procedure | Light condition
--- | --- | ---
Green | Red
1 | Connect red clip to positive battery terminal and black clip to negative battery terminal. | On | Off
2 | Connect connectors A and B of SST (Deployment tool). | Off | On
3 | Press activation switch. | On | Off