#
PCM REMOVAL/INSTALLATION [L3]

BME014018880201

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

European (L.H.D.) specs.

U.K. specs.

1 | Glove compartment
2 | Air duct (See Air Duct Removal Note.)
3 | Set nut (See Set Nut/bolt (U.K. Specs.) Removal Note.) (See Set Nut/bolt (U.K. Specs.) Installation Note.)
4 | PCM bracket
5 | Set bolt (See Set Nut/bolt (U.K. Specs.) Removal Note.) (See Set Nut/bolt (U.K. Specs.) Installation Note.)
6 | PCM connector
7 | PCM

## Air Duct Removal Note

1. Disconnect the front blower resistor connector.

2. Remove the air duct stay fastener.

3. Slide the air duct to the right (European (L.H.D.) specs.) or left (U.K. specs.).

4. Tilt the left side (European (L.H.D.) specs.) or right side (U.K. specs.) down to remove the air duct from the installation place.

## Set Nut/bolt (U.K. Specs.) Removal Note

1. Using a chisel and a hammer, cut a groove on the head of the set nut/bolt so that a screwdriver can be inserted.

2. Loose the set nut/bolt using an impact screwdriver or pliers.

## Set Nut/bolt (U.K. Specs.) Installation Note

1. Install a new set nut/bolt and tighten it until the neck of the nut/bolt is cut.