#
SLIDING DOOR REMOVAL/INSTALLATION

BME091173002W01

  Warning

  • Removing the sliding door without supporting it can be dangerous. The sliding door may fall and injure you. Always perform the following proceder with at least another person.

1. Disconnect the negative battery cable.

2. Remove the rear scuff plate.

3. To remove the center guide rail, remove the trunk side trim.

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

6. Adjust the sliding door. (See SLIDING DOOR ADJUSTMENT.)

1 | Rail protector (See Rail Protector Removal Note.)
2 | Clip (See Clip Removal Note.)
3 | Lower rail guide
4 | Sliding door (See Sliding Door Removal Note.)
5 | Center guide rail

## Rail Protector Removal Note

1. Disengage clip A using a fastener remover.

2. Remove the rail protector.

## Clip Removal Note

1. Push the stopper on the clip in using a flathead screwdriver, and move the clip rearward to remove.

## Sliding Door Removal Note

1. Slide the sliding door rearward, and remove the lower roller of the sliding door from the lower guide rail of the body.

2. Slide the sliding door forward, and remove the upper roller of the sliding door from the upper guide rail of the body.

3. Slide the sliding door rearward, and remove the center roller of the sliding door from the center guide rail of the body.