#
JOINT SHAFT (AJ) ASSEMBLY

BME031325700207

1. Assemble in the order indicated in the table.

1 | Bracket
2 | Bearing (See Bearing Assembly Note.)
3 | Dust seal (differential side) (See Dust Seal (Differential Side) Assembly Note.)
4 | Dust cover
5 | Joint shaft (See Joint Shaft Assembly Note.)
6 | Dust seal (drive shaft side) (See Dust Seal (Drive Shaft Side) Assembly Note.)

## Bearing Assembly Note

1. Install the new bearing using the SST and a press.

  Caution

  • Press the outer race of the bearing.

## Dust Seal (Differential Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new left side dust seal using a press, steel plate and the SST.

  Caution

  • Do not damage the rubber part of the dust cover.

## Joint Shaft Assembly Note

1. Assemble the joint shaft using a press and the SST.

  Caution

  • Support the inner race of the bearing.

## Dust Seal (Drive Shaft Side) Assembly Note

1. Apply grease to the new dust seal lip.

2. Install the new right side dust seal using the SSTs and a press.