#
SELECTOR LEVER INSPECTION

BME051846102201

1. Turn the ignition switch to the ON position.

2. With the brake pedal depressed, verify that there is a "click" at each range when shifted in the pattern shown.

3. Verify that the selector lever can only be shifted as shown in the figure.

4. Verify that the positions of the selector lever and the selector indicator light are aligned.

  • If there is any malfunction, adjust the TR switch and/or selector cable. (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [FN4A-EL].) (See TRANSAXLE RANGE (TR) SWITCH ADJUSTMENT [JA5A-EL].) (See SELECTOR CABLE ADJUSTMENT.)

5. Verify that the vehicle operates in each selected range.